{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["Rekapitulacija","gradb_TK"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":2,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Rekapitulacija","index":0,"n_rows":14,"n_cols":4,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["6.5.6  PROJEKTANTSKI POPIS MATERIALA IN DEL"]
[]
[]
[null,"REKAPITULACIJA"]
[]
["6.5.6.1","Gradbena dela za TK",0,"SIT"]
[]
[]
[]
[null,"SKUPAJ brez DDV:",0,"SIT"]
[]
[null,"DDV 20%",0,"SIT"]
[]
[null,"SKUPAJ z DDV:",0,"SIT"]

{"sheet":"gradb_TK","index":1,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["GRADBENA DELA ZA TK"]
[]
[]
["Št.","Opis","Količina","Enota","Cena/enoto","Vrednost","Cena/enoto","Vrednost"]
[]
[1,"Strojni in deloma ročni izkop kabelskega kanala  v terenu  III. do IV. ktg. dim.(šxv) 0,7x1,15 m v dolžini 30 m",20,"m3",0,0]
[null,"-izdelava podlage iz suhega betona MB20 v debelini 10cm, polaganje PVC cevi premera 4x fi110mm (vključno z distančniki, čepi, tesnili, koleni, ...), obbetoniranje z betonom MB20",3.4,"m3",0,0]
[null,"-zasip s tamponskim gramozom ter nabijanje po slojih 20cm, polaganje PVC opozorilnega traku",14.8,"m3",0,0]
[null,"-odvoz odvečnega materiala do 7km",20,"m3",0,0]
[]
[2,"Strojni in deloma ročni izkop kabelskega kanala  v terenu  III. do IV. ktg. dim.(šxv) 0,7x1,15 m v dolžini 30 m",800,"m3",0,0]
[null,"-izdelava podlage iz suhega betona MB20 v debelini 10cm, polaganje PVC cevi premera 4x fi110mm (vključno z distančniki, čepi, tesnili, koleni, ...), obbetoniranje z betonom MB20",165.5,"m3",0,0]
[null,"-zasip s tamponskim gramozom ter nabijanje po slojih 20cm, polaganje PVC opozorilnega traku",605,"m3",0,0]
[null,"-odvoz odvečnega materiala do 7km",800,"m3",0,0]
[]
[3,"Strojni izkop jame dimenzij 1,4 x 1,4 x 1,2 m za izdelavo jaška v terenu III. do IV. ktg., odvoz odvečnega materiala na deponijo (3,0 m3 x 6)",18,"m3",0,0]
[]
[4,"Izdelava kabelskih jaškov 1,2 x 1,2 m, globine 1,2 m z enojnim LTŽ pokrovom z napisom TELEFON",6,"kos",0,0]
[]
[5,"Strojni izkop jame dimenzij 1,0 x 1,0 x 1,0 m za izdelavo jaška v terenu III. do IV. ktg., odvoz odvečnega materiala na deponijo (1,0 m3 x 31)",31,"m3",0,0]
[]
[6,"Izdelava kabelskih jaškov iz betonske cevi fi 0,8 m, globine 1,0 m z enojnim LTŽ pokrovom in napisom TELEFON",31,"kos",0,0]
[]
[]
[7,"Strojni izkop jame za temelj omarice KRO v terenu III do IV ktg ",2.5,"m3",0,0]
[null,"-odvoz odvečnega materiala do 7km",1,"m3",0,0]
[]
[8,"Dobava in postavitev tipskega betonskega temelja tip STO B dim. 390x150x1600 mm  za omarico KRO,s sidrnimi vijaki, vgrajenim cevnim uvodom s cevjo premera 80 mm, ... ",5,"kos",0,0]
[]
[9,"Dobava rumene PVC cevi f110 mm skupaj z original čepi, vodotesnimi spoji, distančniki, koleni, …",3200,"m",0,0]
[]
[10,"Dobava rumene PVC cevi f63 mm skupaj z original čepi, vodotesnimi spoji, distančniki, koleni, …",200,"m",0,0]
[]
[11,"Dobava in montaža (vkop) pocinkanega valjanca FeZn 25x4mm za ozemljitev prostostoječe kabelske omarice, vključno s križnimi sponkami INOX izvedbe, priključitvami na ozemljilne sisteme, ….",125,"m",0,0]
[]
[12,"Dobava in polaganje PVC opozorilnega traku \"POZOR TELEKOM KABEL\"",1500,"m",0,0]
[]
[13,"Pripravljalna in zaključna dela",3,"%",null,0]
[]
[14,"Drobni material",3,"%",null,0]
[]
[15,"Nepredvidena dela z vpisom v gradbeni dnevnik",5,"%",null,0]
[]
["Skupaj gradbena dela za TK:",{"$nulls":4},0,null,0]