{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["0","cesta"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":3,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"0","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"cesta","index":1,"n_rows":121,"n_cols":7,"rows_kept":121,"cut":false,"hidden":false,"merged":[[26,3,26,4],[27,3,27,4],[28,3,28,4],[29,3,29,4],[30,3,30,4],[31,3,31,4],[32,3,32,4],[33,3,33,4]],"flags":["formulas_cached_only"]}
[]
["5.","POPIS DEL-LOGISTIČNI CENTER NA LETALIŠČU"]
[]
[null,"SKUPNA REKAPITULACIJA"]
[]
["1.","CESTA",null,null,0]
["2.","KANALIZACIJA",null,null,0]
["3.","VODOVOD",null,null,0]
["4.","ELEKTRIKA TER TK VODI",null,null,0]
[]
[null,"SKUPAJ",null,null,0]
[null,"DDV 20%",null,null,0]
[null,"VSE SKUPAJ",null,null,0]
[]
[null,"Opomba: pri vsej postavkah, kjer ni izrecno drugače specificirano, je potrebno "]
[null,"zajeti v cene vsa dela ter dobavo vseh materialov!"]
[]
[]
[]
[]
[]
[null,"POPIS DEL - CESTA"]
[]
[]
[]
[]
[null,"PREDDELA",null,0]
[null,"RUŠITVENA DELA",null,0]
[null,"ZEMELJSKA DELA",null,0]
[null,"ZGORNJI USTROJ",null,0]
[null,"ODVODNJA METEORNIH VOD",null,0]
[null,"PROMETNA SIGNALIZACIJA",null,0]
[null,"NEPREDVIDENA DELA",0.1,0]
[null,"SKUPAJ VREDNOST DEL",null,0]
[]
[]
[1,"PREDDELA"]
[]
["1.1","Zakoličba osi ceste","m1",250,0,null,0]
[]
["1.2","Postavitev in zavarovanje gradbenih","kos",13,0,null,0]
[null,"profilov"]
[]
[null,"PREDDELA SKUPAJ",{"$nulls":4},0]
[]
[2,"RUŠITVENA DELA"]
[]
["2.1","Rušenje obtoječih betonskih robnikov,dimenzije 15/25 cm, dolžine do 1 m,vključno z betonsko posteljico,nakladanjem na vozilo in odvoz v mestno deponijo na razdalji do 3 km","m1",30,0,null,0]
[]
["2.2","Rušenje obstoječega asfalta, debeline do 8 cm, z nakladanjemna vozilo in odvozom v mestnodeponijo na razdalji do 3 km","m2",20,0,null,0]
[]
["2.3","Rezanje asfalta debeline do 15 cm","m1",50,0,null,0]
[]
[null,"RUŠITVENA DELA SKUPAJ",{"$nulls":4},0]
[]
["3","ZEMELJSKA DELA"]
[]
["3.1","Izkop humusa v plasti debeline 40 cm, z odlaganjem na rob izkopa","m3",600,0,null,0]
[]
["3.2","Široki izkop globine do 100 cm, v zemljini III in IV ktg z nakladanjem in odvozom v deponijo na razdalji do 1 km","m3",600,0,null,0]
[]
["3.3","Izkop jame dimenzije 50/50 cm, globine 50 cm, v zemljini III-IV ktg","kos",10,0,null,0]
[]
["3.4","Razstiranje humusa","m2",3000,0,null,0]
[]
["3.5","Planiranje in valjanje zemeljskega planuuma z natančnostjo`+- 2 cm","m2",3000,0,null,0]
[]
[null,"ZEMELJSKA DELA SKUPAJ",{"$nulls":4},0]
[]
[4,"ZGORNJI USTROJ"]
[]
["4.1","Dovoz in vgradnja tamponskega drobljenca 0-32 mm,v plasti debeline 30 cm, z valjanjem in ravnanjem +- 1cm","m3",900,0,null,0]
[]
["4.2","Dovoz in vgradnja jalovine ali drugega nasipnega materijala, v plasteh debeline 25 cm, z valjanjem in ravnanjem +- 1cm","m3",2400,0,null,0]
[]
["4.3","Izdelava nosilne plasti iz bituminiziranega drobljenca 0-22 mm v debelini 5 cm","m2",2300,0,null,0]
[]
["4.4","Izdelava obrabno zaporne plasti BB 0/11s  v debelini 4 cm","m2",2300,0,null,0]
[]
["4.5","Izdelava obrabno zaporne plasti iz bitumenskega betona 0-8 mmv debelini 4 cm (pločnik)","m2",180,0,null,0]
[]
["4.6","Dobava in postavitev betonskih robnikov dim. 15/25 cm, vključnoz betonsko posteljico in fugiranjem rež","m1",500,0,null,0]
[]
["4.7","Dobava in postavitev betonskih robnikov dim. 15/25 cm, vključno z betonsko posteljico in fugiranjem rež - poglobljeni","m1",10,0,null,0]
[]
["4.8","Dobava in postavitev betonskih robnikov dim. 8/20 cm, vključnoz betonsko posteljico in fugiranjem rež","m1",500,0,null,0]
[]
["4.9","Dobava in postavitev betonskih robnikov dim. 8/20 cm, vključnoz betonsko posteljico in fugiranjem rež - poglobljeni","m1",10,0,null,0]
[]
["4.10","Dobava in postavitev betonskih robnikov dim. 15/25 cm, z odprtino, vključno zbetonsko posteljico in fugiranjem rež","kos",9,0,null,0]
[]
[null,"SKUPAJ ZGORNJI USTROJ",{"$nulls":4},0]
[]
[]
["5","ODVODNJA METEORNIH VOD"]
[]
["5.1","Izdelava cestnega požiralnika s peskolovom, iz BC fi 50 cm, L= 2 mz vtokom pod robnikom, vključno z izkopom in odvozom zemljine in zasipom s tamponom, izdelavo priključka na kanalizacijsko cev, potrebnim betonom in LŽ pokrovom IMP 5kN (po detajlu)","kos",9,0,null,0]
[]
["5.2","Izdelava cestnega požiralnika s peskolovom, iz BC fi 50 cm, L= 2 mz vtokom skozi rešetko, vključno z izkopom in odvozom zemljine in zasipom s tamponom, izdelavo priključka na kanalizacijsko cev in potrebnim betonom (po detajlu)","kos",1,0,null,0]
[]
[null,"ODVODNJA METEORNIH VOD SKUPAJ",{"$nulls":4},0]
[]
[6,"PROMETNA SIGNALIZACIJA"]
[]
["6.1","Izdelava temelja iz betona MB20 dimenzije 50/50/50 cm","kos",10,0,null,0]
[]
["6.2","Dobava in vgraditev stebrička zaprometni znak iz vroče cinkane cevi fi 64 mm, dolžine 4 m","kos",10,0,null,0]
[]
["6.3","Dobava in montaža prometnega znaka podloga iz ALU pločevine, znak z odsevno folijo, dolžina stranice 60 cm","kos",10,0,null,0]
[]
["6.4","Dobava in montaža prometnega znaka podloga iz ALU pločevine, znak z odsevno folijo, dolžina stranice 60 cm(dopolnilna tabla)","kos",1,0,null,0]
[]
["6.5","Izdelava tankoslojne neprekinjene označbe z enokomponentno belo barvo,širina črte 12 cm","m1",250,0,null,0]
[]
["6.6","Izdelava tankoslojne neprekinjene označbe z enokomponentno rumenobarvo,širina črte 12 cm","m1",80,0,null,0]
[]
["6.7","Izdelava tankoslojne neprekinjene označbe z enokomponentno belobarvo,širina črte 50 cm","m1",52,0,null,0]
[]
["6.8.","Izvedba potrebne signalizacije za čas gradnje priključka (zavarovanje)"]
[null,null,"kos",1,0,null,0]
[null,"PROMETNA SIGNALIZACIJA SKUPAJ",{"$nulls":4},0]