{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["list1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"list1","index":0,"n_rows":160,"n_cols":6,"rows_kept":160,"cut":false,"hidden":false,"merged":[[2,0,2,5],[0,0,0,5],[1,0,1,5]],"flags":["formulas_cached_only"]}
["KANALIZACIJA  OC POD LETALIŠČEM"]
[]
["REKAPITULACIJA"]
[]
["1.","PREDDELA ",null,null,null,0]
["2.","ZEMELJSKA  DELA",null,null,null,0]
["3.","MONTAŽNA IN BETONSKA DELA",null,null,null,0]
["4.","OSTALA DELA",null,null,null,0]
["5.","NEPREDVIDENA DELA (10%)",null,null,null,0]
[null,"SKUPAJ  ",null,null,null,0]
[null,"DDV 20%",null,null,null,0]
[null,"SKUPAJ  DELA",null,null,null,0]
[]
[null,"Opomba: v popisih je upoštevana tudi dobava treh lovilcev olj, kar pa bi bili dolžni  nabaviti posamezni investitorji!"]
[]
["1.","PREDDELA"]
[]
["1.1.","Zakoličba trase kanalizacije z niveliranjem"]
[null,"-kanal F","m",175,0,0]
[null,"-kanal M","m",235,0,0]
[null,"-kanal D","m",265,0,0]
[]
["1.2.","Zakoličba obstoječih komunalnih naprav"]
[null,"pavšal",null,null,0,0]
[]
["1.3.","Naprava in postavitev gradbenih profilov (na mestih kjer se menja smer ali naklon)"]
[null,"-kanal F","kos",6,0,0]
[null,"-kanal M","kos",6,0,0]
[null,"-kanal D","kos",9,0,0]
[]
["1.4.","Rušenje obstoječega revizijskega jaška iz betona, z nakladanjem in odvozom v deponijo do 5km"]
[null,null,"kos",1,0,0]
["1.5.","Izdelava priključka na obstoječi  AB jašek, za PVC ali PEHD cev do 300 mm"]
[null,null,"kos",1,0,0]
[]
[null,"PREDDELA SKUPAJ:",null,null,null,0]
["2.","ZEMELJSKA DELA"]
[]
["2.1.","Strojni izkop humusa v sloju debeline do 20 cm z odmetom do 2 m."]
[null,"-kanal F","m3",0,0,0]
[null,"-kanal M","m3",0,0,0]
[null,"-kanal D","m3",53,0,0]
[]
["2.2.","Strojni izkop jarkov v III(80%) in IV(10%), V(10%) ktg za kanalizacijo v suhem terenu , širine 1.0 do 2.5 m globine do 3.5 m, naklon brežin 75°, z odlaganjem na rob izkopa."]
[null,"-kanal F","m3",0,0,0]
[null,"-kanal M","m3",0,0,0]
[null,"-kanal D","m3",100,0,0]
[]
["2.3.","Strojni izkop jarkov v III(80%), IV(10%) ter V(10%) ktg za kanalizacijo v suhem terenu , širine 1.0 do 2.5 m globine do 3.5 m, naklon brežin 75°, z nakladanjem na prevozno sredstvo in odvozom na deponijo na razdalji do 4 km"]
[null,"-kanal F","m3",420,0,0]
[null,"-kanal M","m3",360,0,0]
[null,"-kanal D","m3",470,0,0]
[]
["2.4.","Ročni izkop z odmetom na rob, globine do 2 m, na križanjih z ostalimi komunalnimi vodi (ocena 3%)"]
[null,null,"m3",40,0,0]
[]
["2.5.","Črpanje vode iz jarkov med izkopom in montažo s črpalko kapacitete do 1 l/s(Obračun po dejansko porabljenem času)"]
[null,null,"ur",100,0,0]
[]
["2.6.","Planiranje dna rova kanalizacije s točnostjo +/- 1 cm, širina DN + 0,30m"]
[null,"-kanal F","m2",148.75,0,0]
[null,"-kanal M","m2",282,0,0]
[null,"-kanal D","m2",265,0,0]
[]
["2.7.","Dobava in zasip kanalizacijskih cevi in jaškov z drobljencem-jalovino, ter komprimiranje v plasteh po 30 cm (pod voznimi površinami)"]
[null,"-kanal F","m3",240,0,0]
[null,"-kanal M","m3",240,0,0]
[null,"-kanal D","m3",0,0,0]
[]
["2.8.","Zasip kanalizacijskih cevi in jaškov z materialom izkopa ter komprimiranje v plasteh po 30 cm (pod nevoznimi površinami)"]
[null,"-kanal F","m3",150,0,0]
[null,"-kanal M","m3",0,0,0]
[null,"-kanal D","m3",0,0,0]
[]
["2.9.","Zsip drenažnih cevi z granulatom 8/32 mm, komprimiranje v plasteh po 30 cm-z dobavo materiala."]
[null,"-kanal D","m3",380.5,0,0]
[]
["2.10.","Nalaganje in odvoz odvečnega materiala z odvozom na deponijo do 4 km, F=1,25"]
[null,null,"m3",10,0,0]
[]
["2.11.","Humusiranje, planiranje in zatravitev zelenic s humusnim materialom  v sloju debeline 20cm"]
[null,null,"m2",265,0,0]
[]
["2.12.","Profiliranje  jarka nad drenažo (s predhodnim zasutjem z materialom od izkopa) s profilno žlico širine 0.6m in naklonom stranic 1:2"]
[null,null,"m3",53,0,0]
[]
[null,"ZEMELJSKA DELA SKUPAJ:",null,null,null,0]
[]
["3.","MONTAŽNA IN BETONSKA DELA"]
[]
["3.1.","Dobava in polaganje PVC kanalizacijskih cevi SN4 DN200  na betonsko posteljico debeline 10cm s polnim obbetoniranjem po detajlu (0.17 m3/m)"]
[null,"-kanal F","m",175,0,0]
[]
["3.4.","Dobava in polaganje BC kanalizacijskih cevi  DN500  na betonsko posteljico debeline 10cm s polnim obbetoniranjem po detajlu "]
[null,"-kanal M","m",160,0,0]
[]
["3.5.","Dobava in polaganje drenažnih cevi STIDREN DK DN 200 na betonsko posteljico 10 cm in obbetoniranje po detajlu"]
[null,"-kanal D","m",32,0,0]
[]
["3.6.","Dobava in polaganje drenažnih cevi STIDREN DK DN 350 na betonsko posteljico 10 cm in obbetoniranje po detajlu"]
[null,"-kanal D","m",233,0,0]
[]
["3.7.","Dobava in polaganje PVC kanalizacijskih cevi SN4 DN250  na betonsko posteljico debeline 10cm s polnim obbetoniranjem po detajlu "]
[null,null,"m",75,0,0]
[]
["3.8.","Dobava in montaža prefabriciranega poliesterskega jaška svetlega premera 800 mm, vključno z muldo in vtokom in iztokom in posteljico iz betona "]
[null,"`-globine do 2,00 m","kos",4,0,0]
[null,"`-globine od 2,00 do 2,50 m","kos",1,0,0]
[]
["3.9.","Dobava in montaža prefabriciranega poliesterskega kaskadnega jaška svetlega premera 1000 mm,globine 3,7m, vključno z vtokom in iztokom in posteljico iz betona "]
[null,null,"kos",1,0,0]
[]
["3.10.","Dobava in montaža betonskih  revizijskih jaškov DN 600, ter obdelavo mulde in priključkov."]
[null,null,"kos",1,0,0]
[]
["3.11.","Dobava in montaža betonskih  revizijskih jaškov DN 800 z asimetričnim konusom 800/600,  ter obdelavo mulde in priključkov."]
[null,"`-globine do 1,80 m","kos",6,0,0]
[]
["3.12.","Dobava in vgradnja pokrova iz litega železa minimalne nosilnosti 50 kN, preseka 600mm, vključno z AB obročem"]
[null,null,"kos",2,0,0]
[]
["3.13.","Dobava in vgradnja pokrova iz litega železa nosilnosti 150 kN vključno z AB obročem in gumi tesnilom, brez odprtin, preseka 600mm-pod voznimi površinami"]
[null,null,"kos",11,0,0]
[]
["3.14.","Izdelava iztočne glave na BC DN 500 v obstoječ jarek po detajlu"]
[null,null,"kos",1,0,0]
[]
["3.15.","Dobava in vgradnja dodatnega priključka na poliesterskem jašku za cev DN 200"]
[null,null,"kos",10,0,0]
[]
["3.16","Tlakovanje dna ter brežin jarka v kamnu in betonu, debeline 40 cm - po detajlu"]
[null,null,"m2",100,0,0]
["3.17","Podaljšanje obstoječega propusta DN 600 z oobetoniranjem cevi 0.5m3/m"]
[null,null,"m",10,0,0]
["3.18","Izdelava čistilnih jaškov iz cevi DN 350, privarjenih na drenažno cev, globine do 2.5 m s pohodnim betonskim pokrovom"]
[null,null,"kos",8,0,0]
[]
["3.19.","Dobava in montaža tipskega lovilva olj-ustreza Regeneracija, tip Aquareg 30 bp 100","kos",3,0,0]
[]
["3.20","Izdelava iztočne glave na BC DN 600-podaljšanje obstoječega propusta"]
[null,null,"kos",2,0,0]
[]
[null,"MONTAŽNA IN BETONSKA DELA SKUPAJ:",null,null,null,0]
[]
["4.","OSTALA DELA"]
[]
["4.1.","Vnos v kataster komunalnih naprav"]
[null,"pavšal",null,null,0,0]
[]
["4.2.","Preizkus vodotesnosti cevovoda"]
[null,"pavšal",null,null,0,0]
[]
["4.3.","Varnostni načrt ureditve gradbišča"]
[null,null,"kos",1,0,0]
[]
["4.4.","Projekt izvedenih del-POV, kanalizacija+cesta (4 izvodi)"]
[null,null,"kos ",null,0,0]
[]
[]
[null,"OSTALA DELA SKUPAJ:",null,null,null,0]