{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["OBČINA AJDOVŠČINA 2008"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"OBČINA AJDOVŠČINA 2008","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[null,null,"ASFALTERSKA DELA"]
[]
[]
[]
[]
[null,"III.Preplastitev v zaselku Gradišče"]
[null,null," (dolžina 140 m, širine 4,5m)"]
[]
[null,"1.","Rezanje in premaz spoja.","m1",18,null,0]
[]
[null,"2.","Dvig ltž rešetk in pokrovov na novo niveleto.","kom",6,null,0]
[]
[null,"3.","Rezkanje asfalta na spojih in priključkih.","m2",125,null,0]
[]
[null,"4.","Čiščenje in pobrizg starega asfalta.","m2",630,null,0]
[]
[null,"5.","Dobava in strojno vgrajevanje BD 11 v povprečni debelini do 3 cm kot izravnava.","t",47,null,0]
[]
[null,"6.","Dobava in strojno vgrajevanje BB 8 v  debelini  3 cm.","m2",630,null,0]
[]
[null,"7.","Zavarovanje prometa v času gradnje.","kom",1,null,0]
[null,null,"SKUPAJ",null,null,null,0]
[]
[]
[]
[]
[null,null,"REKAPITULACIJA"]
[]
[null,null,"SKUPAJ",null,null,null,0]
[null,null,"ddv",0.2,null,null,0]
[]
[null,null,"VSE SKUPAJ",null,null,null,0]