{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["OBČINA AJDOVŠČINA 2008"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"OBČINA AJDOVŠČINA 2008","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[null,null,"ASFALTERSKA DELA"]
[]
[]
[null,"II.Preplastitev v Vrtovinu"]
[null,null," (dolžina 300 m, širine 4,0m)"]
[]
[null,"1.","Odstranitev travnate ruše in nanosa zemlje iz robov ceste v celotni dolžini in širini do 0,50m z nakladanjem na kamion in odvozom na deponijo do 5 km.","m1",520,null,0]
[]
[null,"2.","Izkop plomb,vključno z asfaltom globine do 30 cm,z nakladanjem materiala na kamion in odvozom na deponijo do 5 km, ravnanjem zemeljskega planuma in zasipom z tamponom ter uvaljanje do potrebne zbitosti.","m2",23,null,0]
[]
[null,"3.","Rezanje in premaz spoja.","m1",38,null,0]
[]
[null,"4.","Dvig ltž rešetk in pokrovov na novo niveleto.","kom",2,null,0]
[]
[null,"5.","Izkop  v terenu 3-4.ktg. z nakladanjem na kamion in odvozom na deponijo do 10 km za izogibališče.","m3",68,null,0]
[]
[null,"6.","Ravnanje in valjanje zemeljskega planuma.","m2",41,null,0]
[]
[null,"7.","Dobava in vgrajevanje tampona  v razširitev z uvaljanjem do potrebne zbitosti.","m3",68,null,0]
[]
[null,"8.","Čiščenje in pobrizg starega asfalta.","m2",1225,null,0]
[]
[null,"9.","Dobava in strojno vgrajevanje BD 11 v povprečni debelini do 3 cm kot izravnava.","t",92,null,0]
[]
[null,"10.","Dobava in strojno vgrajevanje BB 8 v  debelini  3 cm.","m2",1255,null,0]
[]
[null,"11.","Izdelava tamponskih bankin v debelini 6 cm in širine 50 cm.","m1",520,null,0]
[]
[null,"12.","Izdelava enostransko obdelanega  kamnitega zidu, dolžine 10m, višine 1,0m, debeline 0,5m z predhodno izdelavo temelja in vsemi ostalimi deli.","m1",10,null,0]
[]
[null,"13.","Nadvišanje betonske krone na mostu z MB 30 dimenzij 0,5x0,15, komplet z vrtanjem sider, opažanjem, ter vsemi ostalimo deli.","m1",25,null,0]
[]
[null,"14.","Dobava in vgradnja nove cestne odbojne ograje - komplet.","m1",25,null,0]
[]
[null,"15.","Zavarovanje prometa v času gradnje.","kom",1,null,0]
[]
[null,null,"SKUPAJ",null,null,null,0]
[]
[]
[]
[null,null,"REKAPITULACIJA"]
[]
[null,null,"SKUPAJ",null,null,null,0]
[null,null,"ddv",0.2,null,null,0]
[]
[null,null,"VSE SKUPAJ",null,null,null,0]