{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["OBČINA AJDOVŠČINA - GORA"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"OBČINA AJDOVŠČINA - GORA","index":0,"n_rows":118,"n_cols":7,"rows_kept":118,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[null,"I. Batuje - cesta Obrtna cona - do vasi (Sokovih)"]
[null,null,"(na novo asfaltacija  v dolžini cca 120 m, širina 3,00 m)"]
[]
[]
[null,1,"Dobava in vgrajevanje tampona.","m3",80,null,0]
[]
[null,2,"Fino planiranje in valjanje tampona","m2",400,null,0]
[]
[null,3,"Dobava in strojno vgrajevanje BB11 v debelini 6 cm.","m2",360,null,0]
[]
[null,4,"Sekanje in premazi spojev.","m1",7,null,0]
[]
[null,5,"Izdelava tamponskih bankin.","m1",240,null,0]
[]
[null,null,"SKUPAJ",null,null,null,0]
[]
[]
[]
[null," II.Batuje - cesta od igrišča do vrhnjih hiš (Roden)"]
[null,null,"(na novo asfaltacija  v dolžini cca 260 m, širina 4,00 m)"]
[]
[null,1,"Grederiranje cestišča za izravnavo sklonov.","m2",1100,null,0]
[]
[null,2,"Dobava in vgrajevanje tampona.","m3",150,null,0]
[]
[null,3,"Fino planiranje in valjanje tampona","m2",1100,null,0]
[]
[null,4,"Sekanje in premazi spojev.","m1",8,null,0]
[]
[null,5,"Dobava in strojno vgrajevanje BB11 v debelini 6 cm.","m2",1050,null,0]
[]
[null,6,"Izdelava tamponskih bankin.","m1",500,null,0]
[]
[null,null,"SKUPAJ",null,null,null,0]
[]
[]
[null," III. Batuje - doasfaltacija ceste ob zidu proti igrišču in do ekološkega otoka"]
[null,null,"(doasfaltacija šir. 1 m do zidu, v dolžini 110 m in novo v dolžini cca 47 m, širina 3,00 m)"]
[]
[null,1,"Strojna odstranitev humusa in trave v deb. cca 5 cm.","m2",110,null,0]
[]
[null,2,"Sekanje in premazi spojev.","m1",110,null,0]
[]
[null,3,"Grederiranje cestišča za izravnavo sklonov.","m2",150,null,0]
[]
[null,4,"Dobava in vgrajevanje tampona.","m3",30,null,0]
[]
[null,5,"Dobava in strojno vgrajevanje BB11 v debelini 6 cm - za priključke.","m2",260,null,0]
[]
[null,6,"Izdelava tamponskih bankin.","m1",100,null,0]
[]
[]
[null,null,"SKUPAJ",null,null,null,0]
[]
[]
[null," IV. Vrtovin - nadaljevanje asfaltacije ceste proti zgornjemu zaselku"]
[null,null,"(širitev in preplastitev ceste, v dolžini cca 350 m, širina 4,00 m)"]
[]
[null,1,"Izkop za drenažo globine do 1m, širine 0,60m.","m3",30,null,0]
[]
[null,2,"PVC drenažne cevi fi 200mm s filcem.","m1",50,null,0]
[]
[null,3,"Čiščenje robov cestišča, strojno nakladanje in odvoz.","m3",140,null,0]
[]
[null,4,"Sekanje in premazi spojev.","m1",10,null,0]
[]
[]
[null,5,"Dobava in vgrajevanje tampona z uvaljanjem in nabijanjem.","m3",180,null,0]
[]
[null,6,"Čiščenje in pobrizg asfalta.","m2",1200,null,0]
[]
[null,7,"Dobava in strojno vgrajevanje BD11 v povprečni debelini 3 cm kot izravnava.","t",40,null,0]
[]
[null,8,"Dobava in strojno vgrajevanje BB8 v debelini 3 cm.","m2",1400,null,0]
[]
[null,9,"Dobava in strojno vgrajevanje BB11 v debelini 6 cm - za priključke.","m2",150,null,0]
[]
[null,10,"Izdelava asfaltne mulde v deb. 6 cm in širini 50 cm.","m1",250,null,0]
[]
[null,11,"Izdelava tamponskih bankin.","m1",500,null,0]
[]
[null,null,"SKUPAJ",null,null,null,0]
[]
[]
[null," V. Kamnje - razširitev in preplastitev dela ceste pod vasjo "]
[null,null,"(širitev in preplastitev ceste, v dolžini cca 450 m, širina 4,00 m)"]
[]
[]
[null,1,"Čiščenje robov cestišča, strojno nakladanje in odvoz.","m3",100,null,0]
[]
[null,2,"Sekanje in premazi spojev.","m1",10,null,0]
[]
[null,3,"Dobava in vgrajevanje tampona z uvaljanjem in nabijanjem.","m3",70,null,0]
[]
[null,4,"Čiščenje in pobrizg asfalta.","m2",1700,null,0]
[]
[null,5,"Dobava in strojno vgrajevanje BD11 v povprečni debelini 3 cm kot izravnava.","t",50,null,0]
[]
[null,6,"Dobava in strojno vgrajevanje BB8 v debelini 3 cm.","m2",1700,null,0]
[]
[null,7,"Dobava in strojno vgrajevanje BB11 v debelini 6 cm - za priključke.","m2",200,null,0]
[]
[null,8,"Izdelava asfaltne mulde v deb. 6 cm in širini 50 cm.","m1",200,null,0]
[]
[null,9,"Izdelava tamponskih bankin.","m1",700,null,0]
[]
[null,null,"SKUPAJ",null,null,null,0]
[]
[]
[]
[]
[null,null,"REKAPITULACIJA"]
[]
[null,null,"SKUPAJ",null,null,null,0]
[null,null,"ddv",0.2,null,null,0]
[]
[null,null,"VSE SKUPAJ",null,null,null,0]