{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["cesta"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"cesta","index":0,"n_rows":100,"n_cols":7,"rows_kept":100,"cut":false,"hidden":false,"merged":[[12,3,12,4],[13,3,13,4],[6,3,6,4],[7,3,7,4],[8,3,8,4],[9,3,9,4]],"flags":["formulas_cached_only"]}
[]
[null,"POPIS DEL-OBNOVA DOLGE POLJANE"]
[]
[null,"SKUPNA REKAPITULACIJA"]
[]
[]
[null,"PREDDELA",null,0]
[null,"RUŠITVENA DELA",null,0]
[null,"ZEMELJSKA DELA",null,0]
[null,"ZGORNJI USTROJ",null,0]
[null,"METEORNE VODE",null,null,0]
[null,"OSTALA DELA",null,null,0]
[null,"NEPREDVIDENA DELA",0.1,0]
[null,"SKUPAJ VREDNOST DEL",null,0]
[null,"DDV",null,null,0]
[null,"VSE SKUPAJ",null,null,0]
[]
[]
[null,"Opomba: pri vsej postavkah, kjer ni izrecno drugače specificirano, je potrebno "]
[null,"zajeti v cene vsa dela ter dobavo vseh materialov!"]
[]
[]
[null,"Ajdovščina, 3.4.2008"]
[]
[null,"Pripravil: Peter Kete, univ.dipl.inž.grad."]
[]
[]
[1,"PREDDELA"]
[]
["1.1","Zakoličba osi ceste","m1",800,0,null,0]
[]
["1.2","Postavitev in zavarovanje gradbenih","kos",40,0,null,0]
[null,"profilov"]
[]
[null,"PREDDELA SKUPAJ",{"$nulls":4},0]
[]
[2,"RUŠITVENA DELA"]
[]
["2.1","Rušenje obtoječih betonskih robnikov,dimenzije 15/25 cm, dolžine do 1 m,vključno z betonsko posteljico,nakladanjem na vozilo in odvoz v mestno deponijo na razdalji do 3 km","m1",100,0,null,0]
[]
["2.2","Rušenje obstoječega asfalta, debeline do 8 cm, z nakladanjem na vozilo in odvozom v  deponijo na razdalji do 10 km","m2",1500,0,null,0]
[]
["2.3","Rezanje asfalta debeline do 15 cm","m1",30,0,null,0]
[]
[null,"RUŠITVENA DELA SKUPAJ",{"$nulls":4},0]
[]
["3","ZEMELJSKA DELA"]
[]
["3.1","Izkop humusa v plasti debeline 20 cm, z odvozom na gradbiščno deponijo","m3",10,0,null,0]
[]
["3.2","Široki izkop globine do 40 cm, v zemljini III in IV ktg z nakladanjem in odvozom v deponijo na razdalji do 10 km - zamenjava slabo nosilnih temelnih tal","m3",180,0,null,0]
[]
[null,"Izkop jarka za kanalizacijo v terenu III do IV kategorije, globina izkopa do 1m, naklon brežin  750","m3",600,0,null,0]
[]
[]
["3.3.","Razstiranje humusa","m2",100,0,null,0]
[]
["3.4.","Planiranje in valjanje zemeljskega planuuma z natančnostjo`+- 2 cm","m2",2500,0,null,0]
[]
[null,"ZEMELJSKA DELA SKUPAJ",{"$nulls":4},0]
[]
[4,"ZGORNJI USTROJ"]
[]
["4.1","Dovoz in vgradnja tamponskega drobljenca 0-32 mm,v plasti debeline 25 cm, z valjanjem in ravnanjem +- 1cm",null,600,0,null,0]
[]
["4.2","Dovoz in vgradnja jalovine ali drugega nasipnega materijala, v plasteh debeline 25 cm, z valjanjem in ravnanjem +- 1cm","m3",420,0,null,0]
[]
["4.3.","Izdelava obrabno zaporne plasti BB 0/11  v debelini 6 cm","m2",2500,0,null,0]
[]
["4.4.","Izdelava asfaltne mulde, širine 0.5m, BB11 6cm","m",300,0,null,0]
[]
[]
[null,"SKUPAJ ZGORNJI USTROJ",{"$nulls":4},0]
[]
[]
["5","KANALIZACIJA"]
[]
["5.1","Dobava in polaganje PVC cevi SN 4 DN250 na betonsko posteljico debeline 13cm z obbetoniranjem po detajlu (0.20m3/m)-polno obbetonirana","m",400,0,null,0]
[]
["5.2","Zasip kanalizacijskih cevi z kamnitim materilom ter komprimiranje v plasteh po 30 cm"]
[null,null,"m3",600,0,null,0]
[]
["5.3","Dobava in vgradnja PVc jaškov globine do 1.5 m skupaj s pokrovom nosilnosti 250 kn"]
[null,null,"kos",20,0,null,0]
[]
["5.4","Izdelava cestnega požiralnika s peskolovom, iz BC fi 50 cm, L= 2 mz vtokom skozi rešetko, vključno z izkopom in odvozom zemljine in zasipom s tamponom, izdelavo priključka na kanalizacijsko cev in potrebnim betonom (po detajlu)","kos",10,0,null,0]
[]
["5.5","Obnova obstoječih LŽ rešetk v dolžini 4m"]
[null,null,"kos",2,0,null,0]
[]
[null,"KANALIZACIJA  SKUPAJ",{"$nulls":4},0]
[]
["6","OSTALA DELA"]
[]
["6.1.","Obnova obstoječega korita sredi vasi"]
[null,null,"kos",2,0,null,0]
[null,"Postavitev informacijske table"]
[null,null,"kos",1,0,null,0]
[]
[null,"OSTALA DELA SKUPAJ",{"$nulls":4},0]